FOG dual boot imaging (CSCI LW840)

Started with the fog wiki, which states the below requirements to dual boot:

Fsck (from live cd)

And defrag, disk check, sfc /scannow from windows, and a proper shutdown :

shutdown /s /f /t 0